; 
; STMicroelectronics Comunication Device Class driver instalation file
; (C)2006 Copyright STMicroelectronics
; 

[Version] 
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%STM%
LayoutFile=layout.inf

[Manufacturer] 
%MFGNAME%=VirComDevice,NT,NTamd64

[DestinationDirs]
DefaultDestDir = 12

[VirComDevice.NT]
%DESCRIPTION%=DriverInstall,USB\VID_0483&PID_5740

[VirComDevice.NTamd64]
%DESCRIPTION%=DriverInstall,USB\VID_0483&PID_5740

[DriverInstall.NT]
Include=mdmcpq.inf
CopyFiles=FakeModemCopyFileSection
AddReg=DriverInstall.NT.AddReg

[DriverInstall.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,usbser.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[DriverInstall.NT.Services]
AddService=usbser, 0x00000002, DriverServiceInst

[DriverServiceInst]
DisplayName=%SERVICE%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\usbser.sys 

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------


[Strings] 
STM         = "STMicroelectronics"
MFGNAME     = "STMicroelectronics"
DESCRIPTION = "STM Virtual COM Port"
SERVICE     = "USB Virtual COM port"
